**FRITZ!Box 6670 Cable**

* DOCSIS 3.1 router for cable internet
* Channel bonding with 2x2 OFDM (A) and 32x8 SC-QAM
* Mesh Wi-Fi: 2x2, Wi-Fi 7 and Wi-Fi 6
* Wi-Fi speeds: 2.4 GHz: up to 720 Mbit/s, 5 GHz: up to 2,880 Mbit/s
* 1 x 2.5-gigabit LAN/WAN port and 4 LAN ports at 1 Gbit/s
* Telephony via DECT, IP/SIP and 1 analog telephone connection (FXS)
* Built-in tuner for streaming TV signals in the home network
* Smart Home via DECT ULE and Zigbee, prepared for Matter
* FRITZ!OS with parental controls, media server, FRITZ!NAS, Wi-Fi guest access, MyFRITZ! and more
* 1 x USB 2.0 for mobile dongles (5G/4G) as well as storage media and printers

**FRITZ!Box 5690 Pro**

* Powerful integrated fiber optic and DSL router
* Supports the fiber standards: GPON up to 2.5 Gbit/s, AON up to 1 Gbit/s
* Can be used on a fiber optic modem (ONT) with 2.5 Gbit/s (WAN)
* Supports DSL including 35b supervectoring to 250 Mbit/s
* Tri-band Mesh, 4x4 on 2.4 GHz, 5 GHz and 6 GHz / Wi-Fi 7, 6E, 6
* Wi-Fi speeds: 2.4 GHz: up to 1,200 Mbit/s, 5 GHz: up to 5,760 Mbit/s, 6 GHz: up to 11.53 Gbit/s
* 1 x 2.5-gigabit LAN/WAN port and 4 LAN ports at 1 Gbit/s
* Telephony via DECT, IP/SIP and 1 analog telephone connection (FXS)
* Smart Home via DECT ULE and Zigbee, prepared for Matter
* 1 x USB 3.1 for mobile dongles (5G/4G) as well as storage media and printers

**FRITZ!Box 5690 XGS**

* High-speed fiber optic router for up to 10 Gbit/s
* Supports the XGS-PON fiber optic standard
* Can be used on a fiber optic modem (ONT) with 10 Gbit/s (WAN)
* Mesh Wi-Fi, 4x4 on 2.4 GHz and 5 GHz, Wi-Fi 7, 6
* Wi-Fi speeds: 2.4 GHz: up to 1,200 Mbit/s, 5 GHz: up to 5,760 Mbit/s
* 1 x 10-gigabit LAN/WAN port and 4 LAN ports at 1 Gbit/s
* Telephony via DECT, IP/SIP and 1 analog telephone connection (FXS)
* Smart Home via DECT ULE and Zigbee, prepared for Matter
* 1 x USB 3.1 for mobile dongles (5G/4G) as well as storage media and printers